Marking Criteria for Drawings:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Criteria |  Excellent | Good |  Pass |  Needs Improvement |
| Text 10% | All letters touch guidelinesAll letters Upper caseLetters are written correctly All letters are vertical | A few letters miss the guidelinesA few letters not vertical or written incorrectly | Some letters miss guidelines, written incorrectly, or at an angle | Few or no guidelinesMany letters miss guidelines, written correctly (lower case), or not vertical |
| Linework 30% | All lines proper densityAll lines consistent widthAll corners touch | A few lines are darker or lighter than requiredA few areas where lines thickness changes | Some lines are the wrong density | Lines have no consistent densityLines at corners don't touch |
| Measurement 20% | All measurements are accurate and the same as in the diagram given | One change in dimension from the given drawing | More than one difference in dimension | Many errors in measurement  |
| Dimensions 40% | All dimension are drawn properlyAll dimensions are placed in a logical positionLeader lines are used correctly | One or two dimensions could be placed better or errors in extension line use or missing dimensions | 2 or 3 errors in placement or measurement or missing dimensions  | Improper dimensioning practice (didn't follow rules) or many missing dimensions |